{"text_format":"3","workbook":"xls","n_sheets":11,"sheets":["Instruktion","WMP XXX","Mod X 5DI","Mod X 10DI","Mod X 5DO","Mod X 10DO","Mod X 4AI","Mod X 8AI","Mod X 4RTD2","Mod X 3AO","SB Underlag"],"not_rendered":{"images":9,"macros":1,"external_links":1,"defined_names":30,"comments":37},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Instruktion","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"WMP XXX","index":1,"n_rows":53,"n_cols":7,"rows_kept":53,"merged":[[2,1,2,3]],"flags":["formulas_cached_only"]}
["Konfiguration I/O-Kanaler  IMSE WebMaster Pro"]
[]
["Projekt/Anläggn"]
["Enhetsnr -ID: ","WMP-XXX"]
["Placering",null,"Antal I/0 (max 40)",1,null,null,1]
[{"$nulls":3},"(räkn. \"Beteckn\")"]
[]
["Ansluter till\nWMP I/O-Kanal","Beteckn","Beskrivande namn","Not","Not"]
["Temp 1","GT1","GT1 Utetemp",null,"ex. Loggas i kortids och dygns-medel…..",null,1]
["Temp 2",{"$nulls":5},0]
["Temp 3",{"$nulls":5},0]
["Temp 4",{"$nulls":5},0]
["Temp 5",{"$nulls":5},0]
["Temp 6",{"$nulls":5},0]
["Temp 7",{"$nulls":5},0]
["Temp 8",{"$nulls":5},0]
["Analog In 1(U)",{"$nulls":5},0]
["Analog In 2(U)",{"$nulls":5},0]
["Analog In 3(U)",{"$nulls":5},0]
["Analog In 4(U)",{"$nulls":5},0]
["Analog In 5(I)",{"$nulls":5},0]
["Analog In 6(I)",{"$nulls":5},0]
["Analog In 7(I)",{"$nulls":5},0]
["Analog In 8(I)",{"$nulls":5},0]
["Digital In 1®",{"$nulls":3},"OBS! Börja DI konfig. med nr 5. D1-4 kan anv även som räknare.",null,0]
["Digital In 2®",{"$nulls":5},0]
["Digital In 3®",{"$nulls":5},0]
["Digital In 4®",{"$nulls":5},0]
["Digital In 5",{"$nulls":5},0]
["Digital In 6",{"$nulls":5},0]
["Digital In 7",{"$nulls":5},0]
["Digital In 8",{"$nulls":5},0]
["Analog Ut 1",{"$nulls":5},0]
["Analog Ut 2",{"$nulls":5},0]
["Analog Ut 3",{"$nulls":5},0]
["Analog Ut 4",{"$nulls":5},0]
["Analog Ut 5",{"$nulls":5},0]
["Analog Ut 6",{"$nulls":5},0]
["Analog Ut 7",{"$nulls":5},0]
["Analog Ut 8",{"$nulls":5},0]
["Digital Ut 1",{"$nulls":5},0]
["Digital Ut 2",{"$nulls":5},0]
["Digital Ut 3",{"$nulls":5},0]
["Digital Ut 4",{"$nulls":5},0]
["Digital Ut 5",{"$nulls":5},0]
["Digital Ut 6",{"$nulls":5},0]
["Digital Ut 7",{"$nulls":5},0]
["Digital Ut 8",{"$nulls":5},0]
[]
["Eth"]
["RS 485 RJ 12"]
["RS 485"]
["RS 232"]

{"sheet":"Mod X 5DI","index":2,"n_rows":14,"n_cols":7,"rows_kept":14,"flags":["formulas_cached_only"]}
["Konfiguration I/O-Kanaler  Exp modul Z-D-IN "]
[]
["Enhetsnr -ID: ","Sen Z-D-IN"]
["Placering","Mod X 5DI","Antal anv I/0 (max 5 DI)",0,null,null,0]
[{"$nulls":3},"(räkn. \"Beteckn\")"]
[]
["I/O-Kanal","Beteckn","Beskrivande namn","Ansluter till","Anm"]
["Digital In 1",{"$nulls":5},0]
["Digital In 2",{"$nulls":5},0]
["Digital In 3",{"$nulls":5},0]
["Digital In 4",{"$nulls":5},0]
["Digital In 5",{"$nulls":5},0]
[]
["RS485",{"$nulls":3}," WMP XXX -RS485/Modbus exp.IO"]

{"sheet":"Mod X 10DI","index":3,"n_rows":19,"n_cols":7,"rows_kept":19,"flags":["formulas_cached_only"]}
["Konfiguration I/O-Kanaler  Exp modul Z-10-D-IN "]
[]
["Enhetsnr -ID: ","Sen Z-10-D-IN"]
["Placering","Mod X 10DI","Antal anv I/0 (max 10 DI)",0,null,null,0]
[{"$nulls":3},"(räkn. \"Beteckn\")"]
[]
["I/O-Kanal","Beteckn","Beskrivande namn","Ansluter till","Anm"]
["Digital In 1",{"$nulls":5},0]
["Digital In 2",{"$nulls":5},0]
["Digital In 3",{"$nulls":5},0]
["Digital In 4",{"$nulls":5},0]
["Digital In 5",{"$nulls":5},0]
["Digital In 6",{"$nulls":5},0]
["Digital In 7",{"$nulls":5},0]
["Digital In 8",{"$nulls":5},0]
["Digital In 9",{"$nulls":5},0]
["Digital In 10",{"$nulls":5},0]
[]
["RS485",{"$nulls":3}," WMP XXX -RS485/Modbus exp.IO"]

{"sheet":"Mod X 5DO","index":4,"n_rows":14,"n_cols":7,"rows_kept":14,"flags":["formulas_cached_only"]}
["Konfiguration I/O-Kanaler  Exp modul Z-D-OUT"]
[]
["Enhetsnr -ID: ","Sen Z-D-OUT"]
["Placering","Mod X 5DO","Antal anv I/0 (max 5 DO)",0,null,null,0]
[{"$nulls":3},"(räkn. \"Beteckn\")"]
[]
["I/O-Kanal","Beteckn","Beskrivande namn","Ansluter till","Anm"]
["Digital Ut 1",{"$nulls":5},0]
["Digital Ut 2",{"$nulls":5},0]
["Digital Ut 3",{"$nulls":5},0]
["Digital Ut 4",{"$nulls":5},0]
["Digital Ut 5",{"$nulls":5},0]
[]
["RS485",{"$nulls":3}," WMP XXX -RS485/Modbus exp.IO"]

{"sheet":"Mod X 10DO","index":5,"n_rows":23,"n_cols":7,"rows_kept":23,"flags":["formulas_cached_only"]}
["Konfiguration I/O-Kanaler  Exp modul Z-10-D-OUT"]
[]
["Enhetsnr -ID: ","Sen Z-10-D-OUT"]
["Placering","Mod X 10DO","Antal anv I/0 (max 10 DO)",0,null,null,0]
[{"$nulls":3},"(räkn. \"Beteckn\")"]
[]
["I/O-Kanal","Beteckn","Beskrivande namn","Ansluter till","Anm"]
["Digital Ut 1",{"$nulls":5},0]
["Digital Ut 2",{"$nulls":5},0]
["Digital Ut 3",{"$nulls":5},0]
["Digital Ut 4",{"$nulls":5},0]
["Digital Ut 5",{"$nulls":5},0]
["Digital Ut 6",{"$nulls":5},0]
["Digital Ut 7",{"$nulls":5},0]
["Digital Ut 8",{"$nulls":5},0]
["Digital Ut 9",{"$nulls":5},0]
["Digital Ut 10",{"$nulls":3},"Används ej!!",null,0]
[]
["RS485",{"$nulls":3}," WMP XXX -RS485/Modbus exp.IO"]
[]
["Notera! Denna modul har ej fullständigt stöd för alla utgångar. Utgångarna är dessutom av Mosfet typ för max 0,5A "]
["Använding förutsätter alltså i de flesta fall externa hjälprelän. Ersätt hellre denna nödv. antal Z-D-OUT(5utg.) som har"]
["reläutgångar 5A 250VAC"]

{"sheet":"Mod X 4AI","index":6,"n_rows":13,"n_cols":7,"rows_kept":13,"flags":["formulas_cached_only"]}
["Konfiguration I/O-Kanaler  Exp modul Z-4AI"]
[]
["Enhetsnr -ID: ","Sen Z-4AI"]
["Placering","Mod X 4AI","Antal anv I/0 (max 4 AI)",0,null,null,0]
[{"$nulls":3},"(räkn. \"Beteckn\")"]
[]
["I/O-Kanal","Beteckn","Beskrivande namn","Ansluter till","Anm"]
["Analog In 1",{"$nulls":5},0]
["Analog In 2",{"$nulls":5},0]
["Analog In 3",{"$nulls":5},0]
["Analog In 4",{"$nulls":5},0]
[]
["RS485",{"$nulls":3}," WMP XXX -RS485/Modbus exp.IO"]

{"sheet":"Mod X 8AI","index":7,"n_rows":17,"n_cols":7,"rows_kept":17,"flags":["formulas_cached_only"]}
["Konfiguration I/O-Kanaler  Exp modul Z-8AI"]
[]
["Enhetsnr -ID: ","Sen Z-8AI"]
["Placering","Mod X 8AI","Antal anv I/0 (max 8 AI)",0,null,null,0]
[{"$nulls":3},"(räkn. \"Beteckn\")"]
[]
["I/O-Kanal","Beteckn","Beskrivande namn","Ansluter till","Anm"]
["Analog In 1",{"$nulls":5},0]
["Analog In 2",{"$nulls":5},0]
["Analog In 3",{"$nulls":5},0]
["Analog In 4",{"$nulls":5},0]
["Analog In 5",{"$nulls":5},0]
["Analog In 6",{"$nulls":5},0]
["Analog In 7",{"$nulls":5},0]
["Analog In 8",{"$nulls":5},0]
[]
["RS485",{"$nulls":3}," WMP XXX -RS485/Modbus exp.IO"]

{"sheet":"Mod X 4RTD2","index":8,"n_rows":13,"n_cols":7,"rows_kept":13,"flags":["formulas_cached_only"]}
["Konfiguration I/O-Kanaler  Exp modul Z-4RTD2"]
[]
["Enhetsnr -ID: ","Sen Z-4RTD2"]
["Placering","Mod X 4AI","Antal anv I/0 (max 4 AI)",0,null,null,0]
[{"$nulls":3},"(räkn. \"Beteckn\")"]
[]
["I/O-Kanal","Beteckn","Beskrivande namn","Ansluter till","Anm"]
["Temp In 1",{"$nulls":3},"(Ange konfig PT-100,500,1000, NI100)",null,0]
["Temp In 2",{"$nulls":5},0]
["Temp In 3",{"$nulls":5},0]
["Temp In 4",{"$nulls":5},0]
[]
["RS485",{"$nulls":3}," WMP XXX -RS485/Modbus exp.IO"]

{"sheet":"Mod X 3AO","index":9,"n_rows":12,"n_cols":7,"rows_kept":12,"flags":["formulas_cached_only"]}
["Konfiguration I/O-Kanaler  Exp modul Z-3AO"]
[]
["Enhetsnr -ID: ","Sen Z-3AO"]
["Placering","Mod X 3AO","Antal anv I/0 (max 3 AO)",0,null,null,0]
[{"$nulls":3},"(räkn. \"Beteckn\")"]
[]
["I/O-Kanal","Beteckn","Beskrivande namn","Ansluter till","Anm"]
["Analog Out 1",{"$nulls":3},"0/4-20 mA alt. 0-10 alt 0-2 Volt",null,0]
["Analog Out 2",{"$nulls":3},"0/4-20 mA",null,0]
["Analog Out 3",{"$nulls":3},"0/4-20 mA",null,0]
[]
["RS485",{"$nulls":3}," WMP XXX -RS485/Modbus exp.IO"]

{"sheet":"SB Underlag","index":10,"n_rows":10,"n_cols":6,"rows_kept":10,"merged":[[2,1,2,4],[3,1,3,4]],"flags":["formulas_cached_only"]}
[null,"Underlag för skåpbyggnation"]
[]
[null,"Projekt/Anläggn"]
[null,"Antal:"]
[null,1,1,0,1]
[null,"AI","AO","DI","DO","Beskrivning / Notering"]
[null,1,{"$nulls":3},"Instruktion: Markera 1 i aktuell kolumn för varje anslutnings-rad"]
[null,null,1]
[{"$nulls":3}," "]
[{"$nulls":4},1]